LIVRE spécialisé Linux sur HP Integrity : LIVRES/PDF_ou_CHM/Prentice.Hall.Linux.on.HP.Integrity.Servers.A.System.Administrators.Guide.Jul.2004.eBook-DDU.chm

IDENTIFICATION DE  MES  MACHINES :

	J'ai recopié plusieurs fois (en rouge) une lettre correspondante à chaque integrity dans l'encadrement de l'ouverture pour les cartes additionnelles à l'arrière des machines.

La machine détaillée ci-dessous est celle notée "A" (SERIAL DEH454730B).
						  Voir plus bas machine "B" (SERIAL DEH454730A).

Au 24 avril 2010, les 2 machines ci-dessus ont les mêmes versions de BMC/ILO/..., à savoir :

	EFI Boot Manager ver 1.10 [14.62]                    
	  hp server rx2620            
	System Firmware:  4.21 [4651] 
	BMC Version:      4.03        
	MP Version:       E.03.30     

____

IMPORTANT : j'ai découvert tardivement (en regardant les autocollants présents dans le serveur, à proximité des slots mémoire) que l'organisation des mémoires suivait un schéma original.
Pour plus de détail, se reporter dans ce document à la section intitulée "ORGANISATION MÉMOIRE".

AUTRE POINT IMPORTANT : il semble plus que recommandé de refermer (ou tout au moins reposer) le capot de l'ordinateur pour éviter les reboot intempestifs. (Je n'ai pas la certitude que la présence du capot soit un gage de "stabilité" mais pour l'instant, avec le capot reposé, je n'ai plus constaté de reboot indésirable.)
Ce qui est clair, c'est qu'une fois le capot suffisamment bien remis, les ventilateurs baissent sensiblement de régime (avec comme bénéfice un volume sonore moindre).

____

également "raccordable" (avec les identifiants mentionnés ci-après, Admin/Admin ou Oper/Oper) sur la prise série DB25 en 9600-N-8-1. (Consulter éventuellement "Default Console - hp integrity rx2600 Server - 5971-4238.pdf".)

Réglage d'un Mac pour accès "distant" en réseau :
$ sudo -s
# networksetup -listallnetworkservices
	An asterisk (*) denotes that a network service is disabled.
	Bluetooth DUN
	Ethernet
	FireWire
	AirPort
# networksetup -setmanual integrity 10.21.21.21 255.255.255.0 10.21.21.1
# ifconfig en0			# pour vérification
# ping 10.21.21.1		# pour vérification accès HP rx2620-1

MBPDiablo2:~ yannick$ nmap -A 10.21.21.1

Starting Nmap 5.00 ( http://nmap.org ) at 2010-01-16 05:26 CET
Interesting ports on 10.21.21.1:
Not shown: 996 closed ports
PORT    STATE SERVICE    VERSION
22/tcp  open  ssh        HP Integrated Lights Out mpSSH 0.1.0 (protocol 2.0)
23/tcp  open  telnet?
80/tcp  open  http       HP 9000 http service
|_ html-title: Site doesn't have a title (text/html).
443/tcp open  ssl/https?
|_ html-title: HP iLO Login

MBPDiablo2:~ yannick$ ssh 10.21.21.1
Received disconnect from 10.21.21.1: 11:  SSH Disabled          ==> "Feature Not Licensed"

PAR CONTRE accessible en HTTP (redirigé automatiquement vers HTTPS)

MBPDiablo:~ yannick$ telnet 10.21.21.1		# fonctionne, même ordinateur éteint pour
Trying 10.21.21.1...							# peu qu'il soit raccordé au secteur !
Connected to 10.21.21.1.
Escape character is '^]'.

 *************************************************************************
  This is a private system. 
  Do not attempt to login unless you are an authorized user.  
  Any authorized or unauthorized access or use may be monitored and can
  result in criminal or civil prosecution under applicable law.
 *************************************************************************

 *************************************************************************
  Only default users are configured.   
  Use one of the following user/password pairs to login:
  
  Admin/Admin
  Oper/Oper
 *************************************************************************

MP login: Admin
MP password: *****

       Hewlett-Packard Integrated Lights-Out HP Integrity and HP 9000

    (c) Copyright Hewlett-Packard Company 1999-2006.  All Rights Reserved.

                           MP Host Name: rx2620-1

                              Revision E.03.30

 *************************************************************************
                         MP ACCESS IS NOT SECURE
  Default MP users are currently configured and remote access is enabled.
  Modify default users passwords or delete default users (see UC command)
                                    OR
            Disable all types of remote access (see SA command)
 *************************************************************************

 *************************************************************************
                           Your Certificate is expired.
               Use the SO command to generate a new certificate.
 *************************************************************************

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> ^D

Connection closed by foreign host.
MBPDiablo:~ yannick$ ssh 10.21.21.1
Received disconnect from 10.21.21.1: 11:  SSH Disabled

MBPDiablo:~ yannick$ telnet 10.21.21.1
Trying 10.21.21.1...
Connected to 10.21.21.1.
Escape character is '^]'.

 *************************************************************************
  This is a private system. 
  Do not attempt to login unless you are an authorized user.  
  Any authorized or unauthorized access or use may be monitored and can
  result in criminal or civil prosecution under applicable law.
 *************************************************************************

 *************************************************************************
  Only default users are configured.   
  Use one of the following user/password pairs to login:
  
  Admin/Admin
  Oper/Oper
 *************************************************************************

MP login: Admin
MP password: *****

       Hewlett-Packard Integrated Lights-Out HP Integrity and HP 9000

    (c) Copyright Hewlett-Packard Company 1999-2006.  All Rights Reserved.

                           MP Host Name: rx2620-1

                              Revision E.03.30

 *************************************************************************
                         MP ACCESS IS NOT SECURE
  Default MP users are currently configured and remote access is enabled.
  Modify default users passwords or delete default users (see UC command)
                                    OR
            Disable all types of remote access (see SA command)
 *************************************************************************

 *************************************************************************
                           Your Certificate is expired.
               Use the SO command to generate a new certificate.
 *************************************************************************

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> co

        (Use Ctrl-B to return to MP main menu.)

- - - - - - - - - - Prior Console Output - - - - - - - - - -
  0xe00000000120e3c0  im_mountroot+0x60
  0xe000000001628590  DoCalllist+0x3a0
End of Stack Trace

linkstamp:          Tue Mar 04 13:10:35 MET 2008
_release_version:   @(#) $Revision: vmunix:    B11.23_LR FLAVOR=perf Fri Aug 29 22:35:38 PDT 2003 $

sync'ing disks (0 buffers to flush): (0 buffers to flush):
0 buffers not flushed
0 buffers still dirty

- - - - - - - - - - - - Live Console - - - - - - - - - - - -

*** A system crash has occurred. (See the above messages for details.)
*** The system is now preparing to dump physical memory to disk, for use
*** in debugging the crash.

ERROR:  No dump space is configured.  Physical memory will not be dumped.
ERROR:  Configured dump space is insufficient to hold dump metadata.
        Physical memory will not be dumped.
***********************************************************
* ROM Version : 04.21
* ROM Date    : 12/18/2006
* BMC Version :  04.03
***********************************************************
0 0 0x0015B2 0x0000000016122410 boot time event 
1 0 0x0000A4 0x0000000000000000 start memory configuration
0 0 0x0015B2 0x0000000022355658 boot time event 
1 0 0x000014 0x0000000000000000 CPU0 starting cell relocation
1 0 0x000009 0x0000000000000000 CPU0 launch EFI

EFI version 1.10 [14.62]
EFI64 Running on Intel(R) Itanium Processor Family 
EFI 1.10 IPF server rx2620 5.48 [Thu Nov 10 15:08:03 2005] firmware by HP

Copyright (c) 2000-2005 Broadcom Corporation
Broadcom NetXtreme Gigabit Ethernet EFI driver v7.0.10

Loading 'SysROM:Floating-Point Software Assistance Handler'...
-- 'SysROM:Floating-Point Software Assistance Handler' returned Success
Loading 'SysROM:SCSI Bus Driver'...
-- 'SysROM:SCSI Bus Driver' returned Success
Loading 'SysROM:SCSI Tape Driver'...
-- 'SysROM:SCSI Tape Driver' returned Success
Loading device drivers

                   EFI Boot Manager ver 1.10 [14.62]                                                                                                            
OS might use only the primary console set via boot manager or conconfig command
                                                                                                                              
/----------------------------------\  
|       System Overview            |  /----------------------------------\                                                                                    
|            Boot Menu             |  |   hp server rx2620               |                                                                                      | HP-UX Primary Boot: 0/1/1/0.1.0  |  | Serial #:  DEH454730B            |                                                                                      | HP-UX HA Alternate Boot: 0/1...  |  |                                  |                                                                                      | HP-UX Alternate Boot: 0/1/1/...  |  | System Firmware:  4.21 [4651]    |                                                                                      | EFI Shell [Built-in]             |  | BMC Version:      4.03           |                                                                                      | Internal Bootable DVD            |  | MP Version:       E.03.30        |                                                                                      | Core LAN Gb A                    |  | Installed Memory: 4096 MB        |                                                                                      | Core LAN Gb B                    |  |                                  |                                                                                    
| -------------------------------  |  |  CPU  Logical                    | 
| Boot Configuration               |  | Module CPUs   Speed  Status      | 
| System Configuration             |  |    0    1    1.3 GHz Active      | 
| Security Configuration           |  |    1    1    1.3 GHz Active      | 
|                                  |  |                                  | 
\----------------------------------/  |                                  | 
                                      |                                  | 
                                      |                                  | 
                                      \----------------------------------/ 
                                                                             
Use <^|v> to scroll     <ENTER> to Select    <ESC> or <X/x> for Previous Menu  

Scsi(Pun1,Lun0) HP 73.4GST373454LC      HPC2 ( 40 MBytes/sec)                 
Loading.: HP-UX Primary Boot: 0/1/1/0.1.0
Starting: HP-UX Primary Boot: 0/1/1/0.1.0

(C) Copyright 1999-2006 Hewlett-Packard Development Company, L.P.
All rights reserved

HP-UX Boot Loader for IPF  --  Revision 2.029

Press Any Key to interrupt Autoboot
\EFI\HPUX\AUTO ==> boot vmunix -lq
Seconds left till autoboot -   0
AUTOBOOTING...> System Memory = 4074 MB
loading section 0
....................................................... (complete)
loading section 1
.............. (complete)
loading symbol table
loading System Directory (boot.sys) to MFS
....
loading MFSFILES directory (bootfs) to MFS
................
Launching /stand/vmunix
SIZE: Text:27749K + Data:6761K + BSS:7891K = Total:42402K

Console is on a Serial Device
Booting kernel...

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  4074 MB              4074 MB              4074 MB             
Kernel :  4074 MB              4074 MB              4074 MB             
User   :  3627 MB              3159 MB              3171 MB             
-------------------------------------------------------------------------

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> co

        (Use Ctrl-B to return to MP main menu.)

- - - - - - - - - - Prior Console Output - - - - - - - - - -

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  4074 MB              4074 MB              4074 MB             
Kernel :  4074 MB              4074 MB              4074 MB             
User   :  3627 MB              3159 MB              3171 MB             
-------------------------------------------------------------------------

- - - - - - - - - - - - Live Console - - - - - - - - - - - -

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> cm

        (Use Ctrl-B to return to MP main menu.)

[rx2620-1] MP:CM> 

[rx2620-1] MP:CM> he

HE

==== MP Help: Main Menu =======================================================

Hardware Revision a5  Firmware Revision E.03.30 Oct 27 2006,13:43:15

Integrated Lights-Out for HP Integrity and HP 9000 - Management Processor (MP)

                        MP Help System

    Use Ctrl-B to exit MP command interface and return to the main MP menu.

    Enter a command at the help prompt:
           OVerview  : Launch the help overview
           LIst      : Show the list of MP Command Menu commands
           <COMMAND> : Enter the command name for help on individual command
           TOPics    : Show all MP Help topics and commands
           HElp      : Display this screen
           Q         : Quit help

====
MP:HE> li
li
==== MP Help: Command Menu List =============================================

BP  : Reset BMC Passwords               MS  : Modem Status                     
CA  : Configure asynch/serial ports     PC  : Remote Power Control             
DATE: Display Date                      PG  : PaGing parameters setup          
DC  : Default Configuration             PR  : Power Restore Policy Config.     
DF  : Display FRU Information           PS  : Power management module Status   
DI  : DIsconnect users                  RB  : Reset BMC                        
DNS : Configure DHCP and DNS            RS  : Reset System through RST signal  
FW  : Upgrade MP firmware               SA  : Set MP Access                    
HE  : Display Help                      SNMP: Configure SNMP parameters        
ID  : System Information                SO  : Security Options                 
IT  : Modify MP inactivity timeouts     SS  : System processors Status         
LC  : Configure LAN, SSH and Web ports  SYSREV: Display System firmware Revs.  
LDAP: Configure Directory parameters    TC  : Reset system via INIT            
LM  : License Management                TE  : TEll- send a msg. to other users 
LOC : Locator LED display               UC  : User Configuration               
LS  : LAN Status                        WHO : Display connected MP users       
MR  : Modem Reset                       XD  : Diagnostics and reset of MP      

====
(HE for main help, enter command name, or Q to quit)
MP:HE> 

==== MP Help: Main Menu =======================================================

Hardware Revision a5  Firmware Revision E.03.30 Oct 27 2006,13:43:15

Integrated Lights-Out for HP Integrity and HP 9000 - Management Processor (MP)

                        MP Help System

    Use Ctrl-B to exit MP command interface and return to the main MP menu.

    Enter a command at the help prompt:
           OVerview  : Launch the help overview
           LIst      : Show the list of MP Command Menu commands
           <COMMAND> : Enter the command name for help on individual command
           TOPics    : Show all MP Help topics and commands
           HElp      : Display this screen
           Q         : Quit help

====
MP:HE> q
q

[rx2620-1] MP:CM> ldap

LDAP

MP Advanced license is required to use LDAP feature.
Please see Help on "LM" (License Management) for more details.

[rx2620-1] MP:CM> tc

TC

Execution of this command irrecoverably halts all system processing and
I/O activity and restarts the computer system.

Type Y to confirm your intention to restart the system: (Y/[N]) n
n
   -> SPU hardware has not been reset.

[rx2620-1] MP:CM> he

HE

==== MP Help: Main Menu =======================================================

Hardware Revision a5  Firmware Revision E.03.30 Oct 27 2006,13:43:15

Integrated Lights-Out for HP Integrity and HP 9000 - Management Processor (MP)

                        MP Help System

    Use Ctrl-B to exit MP command interface and return to the main MP menu.

    Enter a command at the help prompt:
           OVerview  : Launch the help overview
           LIst      : Show the list of MP Command Menu commands
           <COMMAND> : Enter the command name for help on individual command
           TOPics    : Show all MP Help topics and commands
           HElp      : Display this screen
           Q         : Quit help

====
MP:HE> li
li
==== MP Help: Command Menu List =============================================

BP  : Reset BMC Passwords               MS  : Modem Status                     
CA  : Configure asynch/serial ports     PC  : Remote Power Control             
DATE: Display Date                      PG  : PaGing parameters setup          
DC  : Default Configuration             PR  : Power Restore Policy Config.     
DF  : Display FRU Information           PS  : Power management module Status   
DI  : DIsconnect users                  RB  : Reset BMC                        
DNS : Configure DHCP and DNS            RS  : Reset System through RST signal  
FW  : Upgrade MP firmware               SA  : Set MP Access                    
HE  : Display Help                      SNMP: Configure SNMP parameters        
ID  : System Information                SO  : Security Options                 
IT  : Modify MP inactivity timeouts     SS  : System processors Status         
LC  : Configure LAN, SSH and Web ports  SYSREV: Display System firmware Revs.  
LDAP: Configure Directory parameters    TC  : Reset system via INIT            
LM  : License Management                TE  : TEll- send a msg. to other users 
LOC : Locator LED display               UC  : User Configuration               
LS  : LAN Status                        WHO : Display connected MP users       
MR  : Modem Reset                       XD  : Diagnostics and reset of MP      

====
(HE for main help, enter command name, or Q to quit)
MP:HE> q
q

[rx2620-1] MP:CM> pc

PC

Current System Power State: On 

Power Control Menu:
     C   - Power Cycle
     ON  - Power On
     OFF - Power Off
     G   - Graceful Shutdown

Enter menu item or [Q] to Quit: off
off

System will be powered off.

   You must shut down the OS manually before this command is executed.
   Failure to do this can cause problems when the OS is restarted.
   Confirm? (Y/[N]): y
y

   -> System is being powered off.

[rx2620-1] MP:CM> 

[rx2620-1] MP:CM> 

[rx2620-1] MP:CM> q

Unrecognized Command : Type HE for help on the available commands 

[rx2620-1] MP:CM> 

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> daye

*** Invalid Selection ***

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> date

*** Invalid Selection ***

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> cm

        (Use Ctrl-B to return to MP main menu.)

[rx2620-1] MP:CM> date

DATE

Current Date and Time: 05/10/2009 10:37:19

[rx2620-1] MP:CM> ls

LS

Current LAN Configuration:
     MAC Address                : 0x0015608aaaf8
     DHCP Status                : Disabled 
     IP Address                 : 10.21.21.1
     MP Host Name               : rx2620-1
     Subnet Mask                : 255.255.255.0
     Gateway Address            : 10.21.21.1
     Link State                 : Auto Negotiate
     Remote Serial Console Port : 2023
     SSH Access Port            : - (MP Feature Not Licensed)
     IPMI / LAN Port            : 623

LAN status: UP and RUNNING 

[rx2620-1] MP:CM> df

DF

To dump all available FRU information without any paging, use
the command line interface: DF -ALL -NC

Display FRU Information Menu:
     S - Specific FRU
     A - All available FRUs
     V - Display Mode: Text

Enter menu item or [Q] to Quit: a
a

FRU Entry #   0 : 
FRU NAME: CPU 0 PIROM ID:20

PROCESSOR DATA 
 S-spec/QDF:  SL8CY
 Sample/Prod: 01

CORE DATA 
 Arch Revision                :  00
 Core Family                  :  1F
 Core Model                   :  02
 Core Stepping                :  02
 Max Core Frequency           : 1300 MHZ
 Max SysBus Frequency         :  200 MHZ
 Core Voltage                 : 1150 mV
 Core Voltage Tolerance,High  :   17 mV
 Core Voltage Tolerance,Low   :   17 mV

CACHE DATA 
 Cache Size                   : 3072 KB

PACKAGE DATA 
 Package Revision             : INT3
 Substrate Revision: 00

PROC PART NUMBER DATA 
 Part Number                  : 80543KC
 Electronic Signature         : 000030D0174B2C0E

THERMAL REF DATA 
 Upper Temp Ref               : 101 C
 Calibr Offset                :   0 C

FEATURES DATA 
 IA-32 Proc Core Feature Flags:  FFFB8743
 IA-64 Proc Core Feature Flags:  1B81806300000000
 Package Feature Flags        :  0B000000
 Devices on TAP Chain         :  1

Type <CR> for next entry, or Q to quit: 

FRU Entry #   1 :
FRU NAME: CPU 1 PIROM ID:21

PROCESSOR DATA 
 S-spec/QDF:  SL8CY
 Sample/Prod: 01

CORE DATA 
 Arch Revision                :  00
 Core Family                  :  1F
 Core Model                   :  02
 Core Stepping                :  02
 Max Core Frequency           : 1300 MHZ
 Max SysBus Frequency         :  200 MHZ
 Core Voltage                 : 1150 mV
 Core Voltage Tolerance,High  :   17 mV
 Core Voltage Tolerance,Low   :   17 mV

CACHE DATA 
 Cache Size                   : 3072 KB

PACKAGE DATA 
 Package Revision             : INT3
 Substrate Revision: 00

PROC PART NUMBER DATA 
 Part Number                  : 80543KC
 Electronic Signature         : 0000AD565F25C90B

THERMAL REF DATA 
 Upper Temp Ref               : 101 C
 Calibr Offset                :   0 C

FEATURES DATA 
 IA-32 Proc Core Feature Flags:  FFFB8743
 IA-64 Proc Core Feature Flags:  1B81806300000000
 Package Feature Flags        :  0B000000
 Devices on TAP Chain         :  1

Type <CR> for next entry, or Q to quit: 

FRU Entry #   2 :
FRU NAME: Processor 0 RAM ID:24
Invalid FRU Record Version

Type <CR> for next entry, or Q to quit: q

[rx2620-1] MP:CM> ^[[A

Unrecognized Command : Type HE for help on the available commands 

[rx2620-1] MP:CM> ls

LS

Current LAN Configuration:
     MAC Address                : 0x0015608aaaf8
     DHCP Status                : Disabled 
     IP Address                 : 10.21.21.1
     MP Host Name               : rx2620-1
     Subnet Mask                : 255.255.255.0
     Gateway Address            : 10.21.21.1
     Link State                 : Auto Negotiate
     Remote Serial Console Port : 2023
     SSH Access Port            : - (MP Feature Not Licensed)
     IPMI / LAN Port            : 623

LAN status: UP and RUNNING 

[rx2620-1] MP:CM> df

DF

To dump all available FRU information without any paging, use
the command line interface: DF -ALL -NC

Display FRU Information Menu:
     S - Specific FRU
     A - All available FRUs
     V - Display Mode: Text

Enter menu item or [Q] to Quit: q
q

[rx2620-1] MP:CM> df -all -nc

DF -all -nc

FRU Entry #   0 : 
FRU NAME: CPU 0 PIROM ID:20

PROCESSOR DATA 
 S-spec/QDF:  SL8CY
 Sample/Prod: 01

CORE DATA 
 Arch Revision                :  00
 Core Family                  :  1F
 Core Model                   :  02
 Core Stepping                :  02
 Max Core Frequency           : 1300 MHZ
 Max SysBus Frequency         :  200 MHZ
 Core Voltage                 : 1150 mV
 Core Voltage Tolerance,High  :   17 mV
 Core Voltage Tolerance,Low   :   17 mV

CACHE DATA 
 Cache Size                   : 3072 KB

PACKAGE DATA 
 Package Revision             : INT3
 Substrate Revision: 00

PROC PART NUMBER DATA 
 Part Number                  : 80543KC
 Electronic Signature         : 000030D0174B2C0E

THERMAL REF DATA 
 Upper Temp Ref               : 101 C
 Calibr Offset                :   0 C

FEATURES DATA 
 IA-32 Proc Core Feature Flags:  FFFB8743
 IA-64 Proc Core Feature Flags:  1B81806300000000
 Package Feature Flags        :  0B000000
 Devices on TAP Chain         :  1

FRU Entry #   1 :
FRU NAME: CPU 1 PIROM ID:21

PROCESSOR DATA 
 S-spec/QDF:  SL8CY
 Sample/Prod: 01

CORE DATA 
 Arch Revision                :  00
 Core Family                  :  1F
 Core Model                   :  02
 Core Stepping                :  02
 Max Core Frequency           : 1300 MHZ
 Max SysBus Frequency         :  200 MHZ
 Core Voltage                 : 1150 mV
 Core Voltage Tolerance,High  :   17 mV
 Core Voltage Tolerance,Low   :   17 mV

CACHE DATA 
 Cache Size                   : 3072 KB

PACKAGE DATA 
 Package Revision             : INT3
 Substrate Revision: 00

PROC PART NUMBER DATA 
 Part Number                  : 80543KC
 Electronic Signature         : 0000AD565F25C90B

THERMAL REF DATA 
 Upper Temp Ref               : 101 C
 Calibr Offset                :   0 C

FEATURES DATA 
 IA-32 Proc Core Feature Flags:  FFFB8743
 IA-64 Proc Core Feature Flags:  1B81806300000000
 Package Feature Flags        :  0B000000
 Devices on TAP Chain         :  1

FRU Entry #   2 :
FRU NAME: Processor 0 RAM ID:24
Invalid FRU Record Version

FRU Entry #   3 :
FRU NAME: Processor 1 RAM ID:25
Invalid FRU Record Version

FRU Entry #   4 :
FRU NAME: I/O Backplane ID:05

CHASSIS INFO:

BOARD INFO:
 Mfg Date/Time      : 0
 Manufacturer       : hp
 Product Name       : pci riser card
 S/N                : 40CTQ9F0EK
 Part Number        : A7231-66530
 Fru File ID        : 10
 Custom Info        : A5
 Custom Info        : 4224
 Custom Info        : A5
 Custom Info        : 0

PRODUCT INFO:

FRU Entry #   5 :
FRU NAME: MP Board ID:06

CHASSIS INFO:

BOARD INFO:
 Mfg Date/Time      : 0
 Manufacturer       : hp
 Product Name       : management processor card
 S/N                : 52CTQ86062
 Part Number        : AB587-60002
 Fru File ID        : 10
 Custom Info        : A
 Custom Info        : 4538
 Custom Info        : C
 Custom Info        : 0

PRODUCT INFO:

FRU Entry #   6 :
FRU NAME                : DIMM0A
FRU ID                  : 0x80
JEDEC SPD Rev           : 0x00
JEDEC Mfg ID            : 0x7F94FFFFFFFFFFFF
JEDEC Mfg Location      : 0x02
JEDEC Mfg Part #        : A6969AX-HYICHT0B  
JEDEC Mfg Revision Code : 0x00FF
JEDEC Mfg Year          : 0x05
JEDEC Mfg Week          : 0x44
JEDEC Mfg Serial #      : 0x061D9E18
Mfg Unique Serial #     : 0x0194020544061D9E18

FRU Entry #   7 :
FRU NAME                : DIMM0B
FRU ID                  : 0x81
JEDEC SPD Rev           : 0x00
JEDEC Mfg ID            : 0x7F94FFFFFFFFFFFF
JEDEC Mfg Location      : 0x02
JEDEC Mfg Part #        : A6969AX-HYICHT0B  
JEDEC Mfg Revision Code : 0x00FF
JEDEC Mfg Year          : 0x05
JEDEC Mfg Week          : 0x44
JEDEC Mfg Serial #      : 0x061D9DB1
Mfg Unique Serial #     : 0x0194020544061D9DB1

FRU Entry #   8 :
FRU NAME                : DIMM1A
FRU ID                  : 0x88
JEDEC SPD Rev           : 0x00
JEDEC Mfg ID            : 0x7F94FFFFFFFFFFFF
JEDEC Mfg Location      : 0x02
JEDEC Mfg Part #        : A6969AX-HYICHT0B  
JEDEC Mfg Revision Code : 0x00FF
JEDEC Mfg Year          : 0x05
JEDEC Mfg Week          : 0x44
JEDEC Mfg Serial #      : 0x061D9E96
Mfg Unique Serial #     : 0x0194020544061D9E96

FRU Entry #   9 :
FRU NAME                : DIMM1B
FRU ID                  : 0x89
JEDEC SPD Rev           : 0x00
JEDEC Mfg ID            : 0x7F94FFFFFFFFFFFF
JEDEC Mfg Location      : 0x02
JEDEC Mfg Part #        : A6969AX-HYICHT0B  
JEDEC Mfg Revision Code : 0x00FF
JEDEC Mfg Year          : 0x05
JEDEC Mfg Week          : 0x44
JEDEC Mfg Serial #      : 0x061D9E97
Mfg Unique Serial #     : 0x0194020544061D9E97

FRU Entry #  10 :
FRU NAME: Motherboard ID:00

CHASSIS INFO:
 Type:Rack Mount Chassis

BOARD INFO:
 Mfg Date/Time      : 5188618
 Manufacturer       : CELESTICA 
 Product Name       : motherboard                     
 S/N                : 52CTQA007A      
 Part Number        : AB331-60001
 Fru File ID        : 10
 Custom Info        : B
 Custom Info        : 4521
 Custom Info        : A5
 Custom Info        : 0

PRODUCT INFO:
 Manufacturer       : hp
 Product Name       : server rx2620
 Part/Model         : AB333A
 S/N                : DEH454730B
 FRU File ID        : 11
 Custom Info        : 10a

   -> This is the last entry in the selected list.

-> Command successful.

[rx2620-1] MP:CM> ms

MS

Type <CR> to update modem status, or Q to quit

 -Modem state-  --------------   Remote port Modem Signals   -------------

                RTS/105   DTR/108   CTS/106   DSR/107   DCD/109    RI/125

 Session idle      0         0         0         0         0         0
q

[rx2620-1] MP:CM> ms

MS

Type <CR> to update modem status, or Q to quit

 -Modem state-  --------------   Remote port Modem Signals   -------------

                RTS/105   DTR/108   CTS/106   DSR/107   DCD/109    RI/125

 Session idle      0         0         0         0         0         0

 Session idle      0         0         0         0         0         0

 Session idle      0         0         0         0         0         0
q

[rx2620-1] MP:CM> ps

PS
System Power state: Off           
Temperature       : Low OverTemp  

Power supplies                 State                        
-----------------------------------------------------------
Power Supply 1                Normal                          
Power Supply 2                Normal                          

Fans                           State                        
-----------------------------------------------------------
Fan1A (CPU)                   Normal                         
Fan1B (CPU)                   Normal                         
Fan2 (Memory)                 Normal                         
Fan3 (I/O)                    Normal                         
CPU0 Fan                      Normal                         
CPU1 Fan                      Normal                         

[rx2620-1] MP:CM> co

Unrecognized Command : Type HE for help on the available commands 

[rx2620-1] MP:CM> q

Unrecognized Command : Type HE for help on the available commands 

[rx2620-1] MP:CM> 

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> co

        (Use Ctrl-B to return to MP main menu.)

- - - - - - - - - - Prior Console Output - - - - - - - - - -

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  4074 MB              4074 MB              4074 MB             
Kernel :  4074 MB              4074 MB              4074 MB             
User   :  3627 MB              3159 MB              3171 MB             
-------------------------------------------------------------------------

- - - - - - - - - - - - Live Console - - - - - - - - - - - -

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> cm

        (Use Ctrl-B to return to MP main menu.)

[rx2620-1] MP:CM> sr

SYSREV

Current firmware revisions

 MP FW     : E.03.30
 BMC FW    : 04.03
 EFI FW    : 05.48
 System FW : 04.21

[rx2620-1] MP:CM> ss

SS

System Processor Status:

   System Power is Off.  No processor information is available.

[rx2620-1] MP:CM> who

WHO

User Login        LDAP/Local   Rights         Port Name    IP Address    Mode

Admin              Local      C, P, M, U      LOCAL                       MA   
Admin              Local      C, P, M, U      WEB        10.21.21.216     
Admin              Local      C, P, M, U      TELNET     10.21.21.216     CM   

[rx2620-1] MP:CM> 

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> co

        (Use Ctrl-B to return to MP main menu.)

- - - - - - - - - - Prior Console Output - - - - - - - - - -

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  4074 MB              4074 MB              4074 MB             
Kernel :  4074 MB              4074 MB              4074 MB             
User   :  3627 MB              3159 MB              3171 MB             
-------------------------------------------------------------------------

- - - - - - - - - - - - Live Console - - - - - - - - - - - -

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> se

   -> Request cannot be executed when SPU power is down. 

*** Unable to start a session ***

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> pc

*** Invalid Selection ***

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> cm

        (Use Ctrl-B to return to MP main menu.)

[rx2620-1] MP:CM> pc

PC

Current System Power State: Off 

Power Control Menu:
     C   - Power Cycle
     ON  - Power On
     OFF - Power Off
     G   - Graceful Shutdown

Enter menu item or [Q] to Quit: on
on

System will be powered on.
   Confirm? (Y/[N]): y
y

   -> System is being powered on.

[rx2620-1] MP:CM> 

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> co

        (Use Ctrl-B to return to MP main menu.)

- - - - - - - - - - Prior Console Output - - - - - - - - - -

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  4074 MB              4074 MB              4074 MB             
Kernel :  4074 MB              4074 MB              4074 MB             
User   :  3627 MB              3159 MB              3171 MB             
-------------------------------------------------------------------------

- - - - - - - - - - - - Live Console - - - - - - - - - - - -
***********************************************************
* ROM Version : 04.21
* ROM Date    : 12/18/2006
* BMC Version :  04.03
***********************************************************
0 0 0x0015B2 0x0000000017284851 boot time event 
1 0 0x0000A4 0x0000000000000000 start memory configuration
0 0 0x0015B2 0x0000000023745404 boot time event 
1 0 0x000014 0x0000000000000000 CPU0 starting cell relocation
1 0 0x000009 0x0000000000000000 CPU0 launch EFI

EFI version 1.10 [14.62]
EFI64 Running on Intel(R) Itanium Processor Family 
EFI 1.10 IPF server rx2620 5.48 [Thu Nov 10 15:08:03 2005] firmware by HP

Copyright (c) 2000-2005 Broadcom Corporation
Broadcom NetXtreme Gigabit Ethernet EFI driver v7.0.10

Loading 'SysROM:Floating-Point Software Assistance Handler'...
-- 'SysROM:Floating-Point Software Assistance Handler' returned Success
Loading 'SysROM:SCSI Bus Driver'...
-- 'SysROM:SCSI Bus Driver' returned Success
Loading 'SysROM:SCSI Tape Driver'...
-- 'SysROM:SCSI Tape Driver' returned Success
Loading device drivers

                   EFI Boot Manager ver 1.10 [14.62]                                                                                                            
OS might use only the primary console set via boot manager or conconfig command
                                      /----------------------------------\                                                                                      
/----------------------------------\  |       System Overview            |                                                                                      |            Boot Menu             |  |   hp server rx2620               |                                                                                      | HP-UX Primary Boot: 0/1/1/0.1.0  |  | Serial #:  DEH454730B            |                                                                                      | HP/------------------------------\  |                                  |                                                                                      | HP|    System Configuration      |  | System Firmware:  4.21 [4651]    |                                                                                      | EF| Advanced System Information  |  | BMC Version:      4.03           |                                                                                      | In| Se/------------------------------------\sion:       E.03.30        |                                                                                      | Co| Se|    Advanced System Information     |led Memory: 4096 MB        |                                                                                      | Co| Se| Display All Information            |                           |                                                                                    
| --| Se| System Information                 | ogical                    | 
| Bo| Se| Processor Information              | CPUs   Speed  Status      | 
| Sy| Se| Memory Information                 |  1    1.3 GHz Active      | 
| Se|   | I/O Information                    |  1    1.3 GHz Active      | 
|   \---| Boot Information                   |                           | 
\-----  | Firmware Information               |                           | 
        | Warning and Stop Boot Information  |                           | 
        |v                                   |                           | 
        \------------------------------------/ --------------------------/ 
                                                                             
Use <^|v> to scroll     <ENTER> to Select    <ESC> or <X/x> for Previous Menu  
System Information                                                             

SYSTEM INFORMATION

Date/Time:  May 10, 2009  10:49:20  (20:09:05:10:10:49:20)
Manufacturer:  hp
Product Name:  server rx2620                   
Product Number:  AB333A
Serial Number:  DEH454730B          
UUID:  44BBC0CC-7C13-11DA-BD88-0FEB480AA43F
System Bus Frequency:  200 MHz
Press any key to continue 

                   EFI Boot Manager ver 1.10 [14.62]                                                                                                            

                                      /----------------------------------\                                                                                      
/----------------------------------\  |       System Overview            |                                                                                      |            Boot Menu             |  |   hp server rx2620               |                                                                                      | HP-UX Primary Boot: 0/1/1/0.1.0  |  | Serial #:  DEH454730B            |                                                                                      | HP/------------------------------\  |                                  |                                                                                      | HP|    System Configuration      |  | System Firmware:  4.21 [4651]    |                                                                                      | EF| Advanced System Information  |  | BMC Version:      4.03           |                                                                                      | In| Se/------------------------------------\sion:       E.03.30        |                                                                                      | Co| Se|    Advanced System Information     |led Memory: 4096 MB        |                                                                                      | Co| Se| Display All Information            |                           |                                                                                    
| --| Se| System Information                 | ogical                    | 
| Bo| Se| Processor Information              | CPUs   Speed  Status      | 
| Sy| Se| Memory Information                 |  1    1.3 GHz Active      | 
| Se|   | I/O Information                    |  1    1.3 GHz Active      | 
|   \---| Boot Information                   |                           | 
\-----  | Firmware Information               |                           | 
        | Warning and Stop Boot Information  |                           | 
        |v                                   |                           | 
        \------------------------------------/ --------------------------/ 
                                                                             
Use <^|v> to scroll     <ENTER> to Select    <ESC> or <X/x> for Previous Menu  
Display All Information                                                        

SYSTEM INFORMATION

Date/Time:  May 10, 2009  10:49:24  (20:09:05:10:10:49:24)
Manufacturer:  hp
Product Name:  server rx2620                   
Product Number:  AB333A
Serial Number:  DEH454730B          
UUID:  44BBC0CC-7C13-11DA-BD88-0FEB480AA43F
System Bus Frequency:  200 MHz

PROCESSOR MODULE INFORMATION

           # of               L3      L4      Family/
   CPU     Logical            Cache   Cache   Model         Processor
   Module  CPUs     Speed     Size    Size    (hex.)   Rev  State
   ------  -------  --------  ------  ------  -------  ---  ------------
     0        1      1.3 GHz    3 MB    None   1F/02    A2        Active
     1        1      1.3 GHz    3 MB    None   1F/02    A2        Active

MEMORY INFORMATION

     ---- DIMM A -----  ---- DIMM B -----
Press ENTER to continue, 'q' to exit:
      DIMM   Current     DIMM   Current  
---  ------ ----------  ------ ----------
 0   1024MB     Active  1024MB     Active
 1   1024MB     Active  1024MB     Active
 2    ----               ----            
 3    ----               ----            
 4    ----               ----            
 5    ----               ----            

   Active Memory    : 4096 MB
   Installed Memory : 4096 MB

I/O INFORMATION

BOOTABLE DEVICES

   Order  Media Type  Path
   -----  ----------  ---------------------------------------

Press ENTER to continue, 'q' to exit:
   Seg  Bus  Dev  Fnc  Vendor  Device Slot  
    #    #    #    #     ID      ID     #   Path
   ---  ---  ---  ---  ------  ------  ---  -----------
    00   00   01   00  0x1033  0x0035   XX  Acpi(HWP0002,0)/Pci(1|0)
    00   00   01   01  0x1033  0x0035   XX  Acpi(HWP0002,0)/Pci(1|1)
    00   00   01   02  0x1033  0x00E0   XX  Acpi(HWP0002,0)/Pci(1|2)
    00   00   02   00  0x1095  0x0649   XX  Acpi(HWP0002,0)/Pci(2|0)
    00   20   01   00  0x1000  0x0030   XX  Acpi(HWP0002,100)/Pci(1|0)
    00   20   01   01  0x1000  0x0030   XX  Acpi(HWP0002,100)/Pci(1|1)
    00   20   02   00  0x8086  0x1079   XX  Acpi(HWP0002,100)/Pci(2|0)
    00   20   02   01  0x8086  0x1079   XX  Acpi(HWP0002,100)/Pci(2|1)
    00   40   01   00  0x8086  0x1079   03  Acpi(HWP0002,200)/Pci(1|0)
    00   40   01   01  0x8086  0x1079   03  Acpi(HWP0002,200)/Pci(1|1)
    00   60   01   00  0x1014  0x01A7   02  Acpi(HWP0002,300)/Pci(1|0)
    00   61   04   00  0x1077  0x2312   02  Acpi(HWP0002,300)/Pci(1|0)/Pci(4|0)
    00   61   04   01  0x1077  0x2312   02  Acpi(HWP0002,300)/Pci(1|0)/Pci(4|1)
    00   61   06   00  0x14E4  0x1648   02  Acpi(HWP0002,300)/Pci(1|0)/Pci(6|0)
    00   61   06   01  0x14E4  0x1648   02  Acpi(HWP0002,300)/Pci(1|0)/Pci(6|1)
    00   80   01   00  0x1014  0x01A7   01  Acpi(HWP0002,400)/Pci(1|0)
    00   81   04   00  0x1077  0x2312   01  Acpi(HWP0002,400)/Pci(1|0)/Pci(4|0)
    00   81   04   01  0x1077  0x2312   01  Acpi(HWP0002,400)/Pci(1|0)/Pci(4|1)
    00   81   06   00  0x14E4  0x1648   01  Acpi(HWP0002,400)/Pci(1|0)/Pci(6|0)
    00   81   06   01  0x14E4  0x1648   01  Acpi(HWP0002,400)/Pci(1|0)/Pci(6|1)
    00   E0   01   00  0x103C  0x1290   XX  Acpi(HWP0002,700)/Pci(1|0)
Press ENTER to continue, 'q' to exit:
    00   E0   01   01  0x103C  0x1048   XX  Acpi(HWP0002,700)/Pci(1|1)
    00   E0   02   00  0x1002  0x5159   XX  Acpi(HWP0002,700)/Pci(2|0)

   Fast initialization: Enabled
   System Wake-On-LAN:  Enabled

BOOT INFORMATION

   Monarch CPU:

   Current  Preferred
   Monarch   Monarch
     CPU       CPU
   Module/   Module/
   Logical   Logical   Warnings
   -------  ---------  --------
     0/0       0/0

   AutoBoot: ON - Timeout is : 10 sec

   Boottest:

Press ENTER to continue, 'q' to exit:
   BOOTTEST Settings Default Variable

   OS is not speedy boot aware.

   Selftest     Setting
   ---------    --------------
   early_cpu    Run this test
   late_cpu     Run this test
   platform     Run this test
   chipset      Run this test
   io_hw        Run this test
   mem_init     Run this test
   mem_test     Run this test

   LAN Address Information:

   LAN Address        Path
   -----------------  ----------------------------------------

FIRMWARE INFORMATION

   System Firmware Revision: 4.21 [4651]
Press ENTER to continue, 'q' to exit:
      PAL_A: 7.31/1.27
      PAL_B: 2.15
      EFI Spec: 1.10
      EFI Intel Drop: 14.62
      EFI Build: 5.48
      SAL Spec: 3.01
      SAL_A: 2.00
      SAL_B: 4.21
      POSSE: 0.20
      ACPI: 7.00
      SMBIOS: 2.3.2a
   BMC Revision: 4.03
      IPMI: 1.00
   Management Processor Revision: E.03.30
   Updatable EFI Drivers:
      Floating-Point Software Assistance Handler:  00000118
      LSI Logic Ultra320 SCSI Driver:              01040200
      Broadcom Gigabit Ethernet Driver:            0007000A
      SCSI Bus Driver:                             00000021
      SCSI Tape Driver:                            00000020
      Intel(R) PRO/1000 Ethernet Driver:           00002160
      Usb Ohci Driver:                             00000033
      USB Bus Driver:                              00000014
      USB Bot Mass Storage Driver:                 00000014
Press ENTER to continue, 'q' to exit:
      Generic USB Mass Storage Driver:             00000015

WARNING AND STOP BOOT INFORMATION

CHIP REVISION INFORMATION

   Chip                  Logical     Device       Chip 
   Type                     ID         ID       Revision
   -------------------   -------     ------     --------
   Memory Controller         0       122b         0023 
   Root Bridge               0       1229         0023 
     Host Bridge          0000       122e         0032 
     Host Bridge          0001       122e         0032 
     Host Bridge          0002       122e         0032 
     Host Bridge          0003       122e         0032 
     Host Bridge          0004       122e         0032 
     Host Bridge          0006       122e         0032 
     Host Bridge          0007       122e         0032 
     Other Bridge            0          0         0002 
       Other Bridge          0          0         000d 
         Baseboard MC        0          0         0403 

Press any key to continue 

                   EFI Boot Manager ver 1.10 [14.62]                                                                                                            

                                      /----------------------------------\                                                                                      
/----------------------------------\  |       System Overview            |                                                                                      |            Boot Menu             |  |   hp server rx2620               |                                                                                      | HP-UX Primary Boot: 0/1/1/0.1.0  |  | Serial #:  DEH454730B            |                                                                                      | HP/------------------------------\  |                                  |                                                                                      | HP|    System Configuration      |  | System Firmware:  4.21 [4651]    |                                                                                      | EF| Advanced System Information  |  | BMC Version:      4.03           |                                                                                      | In| Se/------------------------------------\sion:       E.03.30        |                                                                                      | Co| Se|    Advanced System Information     |led Memory: 4096 MB        |                                                                                      | Co| Se| Display All Information            |                           |                                                                                    
| --| Se| System Information                 | ogical                    | 
| Bo| Se| Processor Information              | CPUs   Speed  Status      | 
| Sy| Se| Memory Information                 |  1    1.3 GHz Active      | 
| Se|   | I/O Information                    |  1    1.3 GHz Active      | 
|   \---| Boot Information                   |                           | 
\-----  | Firmware Information               |                           | 
        | Warning and Stop Boot Information  |                           | 
        |v                                   |                           | 
        \------------------------------------/ --------------------------/ 
                                                                             
Use <^|v> to scroll     <ENTER> to Select    <ESC> or <X/x> for Previous Menu  
Memory Information                                                             

MEMORY INFORMATION

     ---- DIMM A -----  ---- DIMM B -----
      DIMM   Current     DIMM   Current  
---  ------ ----------  ------ ----------
 0   1024MB     Active  1024MB     Active
 1   1024MB     Active  1024MB     Active
 2    ----               ----            
 3    ----               ----            
 4    ----               ----            
 5    ----               ----            

   Active Memory    : 4096 MB
   Installed Memory : 4096 MB

Press any key to continue 

                   EFI Boot Manager ver 1.10 [14.62]                                                                                                            

                                      /----------------------------------\                                                                                      
/----------------------------------\  |       System Overview            |                                                                                      |            Boot Menu             |  |   hp server rx2620               |                                                                                      | HP-UX Primary Boot: 0/1/1/0.1.0  |  | Serial #:  DEH454730B            |                                                                                      | HP/-------------------------\..  |  |                                  |                                                                                      | HP|   Boot Configuration    |..  |  | System Firmware:  4.21 [4651]    |                                                                                      | EF| Boot From File          |    |  | BMC Version:      4.03           |                                                                                      | In| Add Boot Entry          |    |  | MP Version:       E.03.30        |                                                                                      | Co| Edit Boot Entry         |    |  | Installed Memory: 4096 MB        |                                                                                      | Co| Remove Boot Entry       |    |  |                                  |                                                                                    
| --| Edit OS Boot Order      | -  |  |  CPU  Logical                    | 
| Bo| AutoBoot Configuration  |    |  | Module CPUs   Speed  Status      | 
| Sy| BootNext Configuration  |    |  |    0    1    1.3 GHz Active      | 
| Se| ----------------------  |    |  |    1    1    1.3 GHz Active      | 
|   | Driver Configuration    |    |  |                                  | 
\---| Console Configuration   | ---/  |                                  | 
    | ----------------------  |       |                                  | 
    |v                        |       |                                  | 
    \-------------------------/       \----------------------------------/ 
                                                                             
Use <^|v> to scroll     <ENTER> to Select    <ESC> or <X/x> for Previous Menu  
Add Boot Entry                                                                 

Searching for devices
Scsi(Pun0,Lun0) HP 73.4GST373454LC      HPC2 (320 MBytes/sec)                 
Scsi(Pun1,Lun0) HP 73.4GST373454LC      HPC2 ( 40 MBytes/sec)                 
HP 2Port 2Gb Fibre Channel Adapter (driver 1.47, firmware 3.03.154)  
HP 2Port 2Gb Fibre Channel Adapter (driver 1.47, firmware 3.03.154)  
Broadcom NetXtreme Gigabit Ethernet (BCM5704) is detected (PCI-X)
Broadcom NetXtreme Gigabit Ethernet (BCM5704) is detected (PCI-X)
HP 2Port 2Gb Fibre Channel Adapter (driver 1.47, firmware 3.03.154)  
HP 2Port 2Gb Fibre Channel Adapter (driver 1.47, firmware 3.03.154)  
Broadcom NetXtreme Gigabit Ethernet (BCM5704) is detected (PCI-X)
Broadcom NetXtreme Gigabit Ethernet (BCM5704) is detected (PCI-X)

                   EFI Boot Manager ver 1.10 [14.62]                                                                                                            
OS might use only the primary console set via boot manager or conconfig command
                                      /----------------------------------\                                                                                      
/----------------------------------\  |       System Overview            |                                                                                      |            Boot Menu             |  |   hp server rx2620               |                                                                                      | HP-UX Primary Boot: 0/1/1/0.1.0  |  | Serial #:  DEH454730B            |                                                                                      | HP-UX HA Alternate Boot: 0/1...  |  |                                  |                                                                                      | HP-UX Alternate Boot: 0/1/1/...  |  | System Firmware:  4.21 [4651]    |                                                                                      | EFI Shell [Built-in]             |  | BMC Version:      4.03           |                                                                                      | Internal Bootable DVD            |  | MP Version:       E.03.30        |                                                                                      | Core LAN Gb A                    |  | Installed Memory: 4096 MB        |                                                                                      | Core LAN Gb B                    |  |                                  |                                                                                    
| -------------------------------  |  |  CPU  Logical                    |    
| Boot Configuration               |  | Module CPUs   Speed  Status      |    
| System Configuration             |  |    0    1    1.3 GHz Active      |    
| Security Configuration           |  |    1    1    1.3 GHz Active      |    
|                                  |  |                                  |  | 
\----------------------------------/ (|                                  |  | 
                                     (|                                  |  | 
   |                                  |                                  |  | 
   \                            ------\----------------------------------/ -/ 
                                                                                
Use <^|v> to scroll     <ENTER> to Select    <ESC> or <X/x> for Previous Menu  

Loading.: HP-UX Primary Boot: 0/1/1/0.1.0
Starting: HP-UX Primary Boot: 0/1/1/0.1.0

(C) Copyright 1999-2006 Hewlett-Packard Development Company, L.P.
All rights reserved

HP-UX Boot Loader for IPF  --  Revision 2.029

Press Any Key to interrupt Autoboot
\EFI\HPUX\AUTO ==> boot vmunix -lq
Seconds left till autoboot -   0
AUTOBOOTING...> System Memory = 4074 MB
loading section 0
....................................................... (complete)
loading section 1
.............. (complete)
loading symbol table
loading System Directory (boot.sys) to MFS
....
loading MFSFILES directory (bootfs) to MFS
................
Launching /stand/vmunix
SIZE: Text:27749K + Data:6761K + BSS:7891K = Total:42402K

Console is on a Serial Device
Booting kernel...

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  4074 MB              4074 MB              4074 MB             
Kernel :  4074 MB              4074 MB              4074 MB             
User   :  3627 MB              3159 MB              3171 MB             
-------------------------------------------------------------------------

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> co

        (Use Ctrl-B to return to MP main menu.)

- - - - - - - - - - Prior Console Output - - - - - - - - - -

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  4074 MB              4074 MB              4074 MB             
Kernel :  4074 MB              4074 MB              4074 MB             
User   :  3627 MB              3159 MB              3171 MB             
-------------------------------------------------------------------------

- - - - - - - - - - - - Live Console - - - - - - - - - - - -

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> pc

*** Invalid Selection ***

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> cm

        (Use Ctrl-B to return to MP main menu.)

[rx2620-1] MP:CM> pc

PC

Current System Power State: On 

Power Control Menu:
     C   - Power Cycle
     ON  - Power On
     OFF - Power Off
     G   - Graceful Shutdown

Enter menu item or [Q] to Quit: g
g

System will be gracefully shutdown.
   Confirm? (Y/[N]): y
y

   -> System has been requested graceful shutdown.

[rx2620-1] MP:CM> co

Unrecognized Command : Type HE for help on the available commands 

[rx2620-1] MP:CM> 

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> co

        (Use Ctrl-B to return to MP main menu.)

- - - - - - - - - - Prior Console Output - - - - - - - - - -

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  4074 MB              4074 MB              4074 MB             
Kernel :  4074 MB              4074 MB              4074 MB             
User   :  3627 MB              3159 MB              3171 MB             
-------------------------------------------------------------------------

- - - - - - - - - - - - Live Console - - - - - - - - - - - -

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> co

        (Use Ctrl-B to return to MP main menu.)

- - - - - - - - - - Prior Console Output - - - - - - - - - -

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  4074 MB              4074 MB              4074 MB             
Kernel :  4074 MB              4074 MB              4074 MB             
User   :  3627 MB              3159 MB              3171 MB             
-------------------------------------------------------------------------

- - - - - - - - - - - - Live Console - - - - - - - - - - - -

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> 

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> cm

        (Use Ctrl-B to return to MP main menu.)

[rx2620-1] MP:CM> pc -?

PC -?

Usage:  PC [ -on | -off | -graceful | -cycle ] [ -nc ]
        PC -?

-> Command successful.

[rx2620-1] MP:CM> pc -off -nc

PC -of fff -nc

** Parse Error: Keyword does not allow a value **

Usage:  PC [ -on | -off | -graceful | -cycle ] [ -nc ]
        PC -?

-> Command failed.

[rx2620-1] MP:CM> pc -off -nc

PC -off -nc

System will be powered off.

   You must shut down the OS manually before this command is executed.
   Failure to do this can cause problems when the OS is restarted.

   -> System is being powered off.

-> Command successful.

[rx2620-1] MP:CM> 

   MP MAIN MENU:

         CO: Console
        VFP: Virtual Front Panel
         CM: Command Menu
         CL: Console Log
         SL: Show Event Logs
         HE: Main Help Menu
          X: Exit Connection

[rx2620-1] MP> x
                Connection closed by foreign host.
MBPDiablo:~ yannick$ 

___________________________________
___________________________________
___________________________________		APRÈS AJOUT RAM (acquise chez SQP en mai 2009)
___________________________________

je démarre la machine avec 

pc -on

Le menu (bleu/blanc) s'affiche et je choisi de démarrer EFI

(REMARQUE : j'avais tenté de démarrer sur "Internal Bootable DVD" mais malgré l'insertion d'un CD memtest86 puis d'un DVD Live de Fedora 10 MAIS rien n'y a fait, aucun n'était jugé "bootable" : 
	Loading.: Internal Bootable DVD
	Load of Internal Bootable DVD failed: Not Found
	Press any key to continue 
)

Shell> fs1:						###  IMPORTANT : sur fs2: (et non fs1:) sur serveur "A"

fs1:\> cd EFI\BOOT				###  REMARQUE : ce "système" N'est PAS case-sensitive !

fs1:\EFI\BOOT> ls
Directory of: fs1:\EFI\BOOT

  11/29/05  05:39a <DIR>          4,096  .
  11/29/05  05:39a <DIR>          4,096  ..
  11/29/05  05:39a              664,064  BOOTIA64.EFI
  11/29/05  05:39a                5,238  IO.INI
  11/29/05  05:39a              664,064  LaunchMenu.efi
  11/29/05  05:39a                4,643  LaunchMenu.ini
  11/29/05  05:39a                4,892  VIEW_DOC.INI
          5 File(s)   1,342,901 bytes
          2 Dir(s)

fs1:\EFI\BOOT> LaunchMenu.efi
HP Itanium Processor Family Diagnostics and Utilities CD        Version A.01.15 

  This CD provides diagnostic applications and tools to support and maintain
  HP systems based on the Intel IPF platform.
  Type the key which corresponds to your selection below:

  a. View CD Overview

  b. Run the Off-line Diagnostic Environment (ODE)

  c. Run CD Installer to install/update CD content to HPSP

  d. View Release Notes and Documentation Menu

  e. View I/O Cards FW Update and Configuration Utilities, MCA, and ICM Menu

  f. View License and Warranty Agreements Notice

  x. exit and reboot          q. exit menu without reboot

J'OPTE POUR LE CHOIX b

***************************************************************************
******                                                               ******
******             Offline Diagnostic Environment                    ******
******                                                               ******
******  (C) Copyright Hewlett-Packard Co 1993-2005                   ******
******                    All Rights Reserved                        ******
******                                                               ******
******  HP shall not be liable for any damages resulting from the    ******
******  use of this program.                                         ******
******                                                               ******
******                TC  Version B.00.18                            ******
******                SysLib Version B.00.09                         ******
******                Mapfile Version B.01.27                        ******
******                                                               ******
***************************************************************************

Type HELP for command information.
ODE> help

	:

ODE> ls

          Modules on this boot media are:

filename      type   size     created   description
-----------------------------------------------------------------------------
CIODIAG2.EFI  TM     731648   11/29/2005  Core IO diagnostic 
COPYUTIL.EFI  TM     1072128  11/29/2005  Disk-to-tape copy utility
CPUDIAG.EFI   TM     819200   11/29/2005  Processor diagnostic
DFDUTIL.EFI   TM     880640   11/29/2005  Disk firmware download utility
FCFUPDATE.EFI TM     279552   11/29/2005  FW Update Utility for Fibre Channel
IODIAG.EFI    TM     183296   11/29/2005  Runs selftests on I/O modules
MAPPER.EFI    TM     1025536  11/29/2005  System mapping utility
MEMDIAG.EFI   TM     291840   11/29/2005  Memory diagnostic
PERFVER.EFI   TM     853504   11/29/2005  Runs ROM-based selftests on peripherals
PLUTODIAG.EFI TM     609280   11/29/2005  SBA/LBA diagnostic

ODE> memdiag

Type HELP for command information.

Please wait, detecting if a MP system.... 
Initializing MP Protocol Interface....
Done
Number of Processors = 2
Total Memory Available For Testing = 8120 MB
Total Chunks  34 
SMBIOS Init successful 

MEMDIAG> help

MEMDIAG Help

     Commands
     --------
     SECTION -- Displays/Sets current test sections to execute
     DIAGINFO -- Displays the test sections covered by memdiag
     UP -- Utilize only one processor
     MP -- Utilize all processors in a system
     MAP -- Displays the memory subsystem 

Continue ([y]/n)? 

ODE Commands Available from MEMDIAG

    Basic Commands
    --------------
    HELP -- Prints detailed information to the screen, when "help <command>"
            or "help <var>" is typed
    LS -- List modules available on boot medium
    <Module_Name> -- Load and initialize a module by typing its name
                     (For more help, type "help module_name")
    RUN -- Run a module (after setting desired environment variables)
    Control-Y|Control-C -- Abort an ODE command; pause a module run
    RESUME -- Restart a paused module
    DISPLOG -- After running a module, display contents of a log
    EXIT -- Return to next higher level prompt

    Environmental Variables
    -----------------------
    SHOWSTATE -- Display the value of the following environment variables:
        LOOP -- Run a test this many times
        ERRPRINT [ON|OFF] -- Print low-level error messages to console
                             (primarily for manufacturing use)
        ERRNUM [ON|OFF] -- Print one-line, numbered errors to the console
        ERRPAUSE [ON|OFF] -- Pause module upon error detection
Continue ([y]/n)? 

        ERRONLY [ON|OFF] -- Print ONLY error messages; disable non-error
                            and isolation message printing
        INFOPRINT [ON|OFF] -- Print informational messages to the console
        ISOPRINT [ON|OFF] -- Print fault isolation messages to the console
        ISOPAUSE [ON|OFF] -- Pause module when isolation message is generated
    LOGSIZE -- Set the size of a message log
    DEFAULT -- Reset environment variables to default state
    SAVE -- Save the content of the error log to a file

MEMDIAG> run

STARTING EXECUTION OF MEMDIAG

SECTION 001
Refresh Test Section

Started Date : 05/17/2009  Time : 12:24:39

Sent AP(1) Start Message
...................................
Finished Date : 05/17/2009  Time : 12:25:38

SECTION 002
Read Hammer Write Test Section

Started Date : 05/17/2009  Time : 12:25:38

Sent AP(1) Start Message
...................................
Finished Date : 05/17/2009  Time : 12:25:51

		:

___________________________

Démarrage "contrôlé" en résumé :

telnet 10.21.21.1
Login:
Password:
cm
	pc -on
	^B
co
	-> attendre apparition menus

ET SI C'EST POUR INTERVENIR SUR LE BOOT HP-UX ALORS LAISSER PASSER L'ETAPE DES MENUS POUR ENSUITE ATTENDRE L'APPARITION DU MESSAGE :

	Press Any Key to interrupt Autoboot

ET PRESSER DONC UNE TOUCHE POUR OBTENIR LE PROMPT SUIVANT :

   Type 'help' for help

HPUX> help
 -- HPUX bootloader for IPF Help --

   -------- supported commands ---------
   boot [kernel]      - boots HPUX kernel
   help [-d]          - help screen (-d to list debug commands)
   mmap               - show current EFI memory map
   ls [-aRdnlogrtucpFLis] [path...]
   ll [-aRdnlogrtucpFLis] [path...] (same as ls -alF)
   setauto [-d] [str] - sets AUTO file (-d to delete AUTO file)
   showauto           - shows AUTO file
   ver                - prints version numbers
   exit               - exits bootloader

HPUX> 

Trouvé dans des pages sur Internet (avec la recherche Google "hp-ux +ia64 reset root password") :
	http://forums11.itrc.hp.com/service/forums/questionanswer.do?threadId=186244

HPUX> hpux -is
> System Memory = 8171 MB
loading section 0
....................................................... (complete)
loading section 1
.............. (complete)
loading symbol table
loading System Directory (boot.sys) to MFS
....
loading MFSFILES directory (bootfs) to MFS
................
Launching /stand/vmunix
SIZE: Text:27749K + Data:6761K + BSS:7891K = Total:42402K

Console is on a Serial Device
Booting kernel...

Memory Class Setup
-------------------------------------------------------------------------
Class     Physmem              Lockmem              Swapmem
-------------------------------------------------------------------------
System :  8171 MB              8171 MB              8171 MB             
Kernel :  8171 MB              8171 MB              8171 MB             
User   :  7536 MB              6566 MB              6592 MB             
-------------------------------------------------------------------------

		===>  À CE STADE, IL FAUT PATIENTER QUELQUES MINUTES AVANT DE VOIR APPARAîTRE LA SUITE.

		:

insf: Installing special files for ipmi instance 0 address 250/0

INIT: Overriding default level with level 's'

INIT: SINGLE USER MODE

INIT: Running /sbin/sh
# 

# fsck
# mount -a -F vxfs
# passwd

# cat fstab
# System /etc/fstab file.  Static information about the file systems
# See fstab(4) and sam(1M) for further details on configuring devices.
/dev/vg00/lvol3 / vxfs delaylog 0 1
/dev/vg00/lvol1 /stand vxfs tranflush 0 1
/dev/vg00/lvol4 /tmp vxfs delaylog 0 2
/dev/vg00/lvol5 /home vxfs delaylog 0 2
/dev/vg00/lvol6 /opt vxfs delaylog 0 2
/dev/vg00/lvol7 /usr vxfs delaylog 0 2
/dev/vg00/lvol8 /var vxfs delaylog 0 2
/dev/vg00/lv_bmc        /bmc    vxfs delaylog 0 2
/dev/vg00/lv_oracle     /oracle vxfs delaylog 0 2
#Swap pour SAP
/dev/vg00/lv_swap       ...     swap default  0 0

# NFS
frbpct13s:/HP           /HP                     nfs  bg,soft 0 2

___ BASCULEMENT ENTRE CONSOLE telnet ET CONSOLE web :

Au message :

 [Read only - use Ctrl-Ecf for console write access.]

Procéder ainsi :

  To execute the ^Ecf command complete the following steps:
	1.	Press the Cntrl key and the e key simultaneously.
	2.	Release the Cntrl key and the e key.
	3.	Press the c key.
	4.	Press the f key.

-------------------------------------------------------------------------

QUELQUES MANIPULATIONS SUR LE HP-UX DONT J'AI REINITIALISE LE MOT DE PASSE root :

Préconisations :
	stty erase ^?
	set -o emacs
	TERM=vt100

srvu0118:/home/root # netstat -i
Name      Mtu  Network         Address         Ipkts   Ierrs Opkts   Oerrs Coll
lan1      1500 10.3.142.0      srvu0118s       57      0     70      0     0   
lan0*     1500 10.3.140.0      srvu0118        1449    0     1449    0     0   
lo0       4136 loopback        localhost       10102   0     10102   0     0   
lan6*     1500 10.3.144.0      srvu0118i       13      0     13      0     0   

srvu0118:/home/root # ifconfig lan1
lan1: flags=1843<UP,BROADCAST,RUNNING,MULTICAST,CKO>
        inet 10.3.142.118 netmask ffffff00 broadcast 10.3.142.255

srvu0118:/home/root # ifconfig lan0
lan0: flags=842<BROADCAST,RUNNING,MULTICAST>
        inet 10.3.141.118 netmask fffffe00 broadcast 10.3.141.255

srvu0118:/home/root # ifconfig lan6
lan6: flags=8d2<BROADCAST,POINTOPOINT,RUNNING,NOARP,MULTICAST>
        inet 10.3.144.218 --> 0.0.0.0 netmask ffffff00 broadcast 10.3.144.255

srvu0118:/etc # sam								# pour voir et plus tard modifier !

srvu0118:/etc # lanshow
                  ----------------------------------------- 
                 |                                         | 
                 |         lanshow ( Version:     3.2 )    |
                 |                                         | 
                 |    This tool is for HP support only     | 
                  ----------------------------------------- 

Note: HP CONFIDENTIAL
libp4 (9.293): Opening /stand/current/vmunix /dev/kmem

Loading symbols from /stand/current/vmunix
Kernel TEXT pages not requested in crashconf
Will use an artificial mapping from a.out TEXT pages
Loading symbols from /stand/current/mod/acdd
Loading symbols from /stand/current/mod/atdd
Loading symbols from /stand/current/mod/pfil
Loading symbols from /stand/current/mod/ipf
Loading symbols from /stand/current/mod/rng
Loading symbols from /stand/current/mod/gvid_info
Loading symbols from /stand/current/mod/tsmoptc
Loading symbols from /stand/current/mod/tsmchgr
Loading symbols from /stand/current/mod/tsmtape

Executing:  /usr/contrib/bin/lanshow-a-i  

Loading symbols from /usr/contrib/bin/lanshow_dbg/xport_1123.o

INFORMATION    : SAFER Enablement Patch, PHKL_32798, is installed.
                 Some structure definitions like tcp_t are being
                 imported from the companion binary,
                    lanshow_dbg/xport_1123.o
                 to get the structure for PHNE_37395
Loading symbols from /usr/contrib/bin/lanshow_dbg/msi_debug_1123_ia64.o

Name   PPA   Driver      Interface           Mac       States       IP     
              Name      Description        Address    Link IP     Address  
--------------------------------------------------------------------------------
lan0    0    iether  1000Base-T  Core   0x0016353e0c1c DOWN DOWN 10.3.141.118 
lan1    1    iether  1000Base-T  Core   0x0016353e0c1d UP   UP   10.3.142.118 
lan8    8    igelan  1000Base-T         0x0014c254c9f4 DOWN n/c  n/c          
lan9    9    igelan  1000Base-T         0x0014c254c9f5 DOWN n/c  n/c          
lan10   10   iether  1000Base-T         0x00156004506a DOWN n/c  n/c          
lan11   11   iether  1000Base-T         0x00156004506b DOWN n/c  n/c          

n/c : means "Not Configured", ifconfig has not been done on this interface

srvu0118:/etc # sam								# pour modifier !

# # À NOTER QUE lsof est aussi installé (dans /usr/contrib/bin) !
# # top est fournie en "standard" (nécessite TERM=vt100)

Possibilité de se connecter en HTTP sur le port 2301 (ou alternativement directement en HTTPS sur le port 2381) pour accéder à une interface d'administration Web de la machine.
On peut s'y authentifier en tant que "root".

srvu0118:/etc # vi /opt/ssh/etc/sshd_config
	# déjà sur "Protocol 2" exclusivement
	Port 22001
	PermitRootLogin no

# # À titre anecdotique (quand le temps me le permettra), regarder /opt/ssh/ssh_chroot_setup.sh

srvu0118:/sbin/rc2.d # who -r
   .       run-level 3  Jan 17 05:37    3    0    S

srvu0118:/sbin/rc2.d # ls -l /sbin/rc2.d/S393secsh 
lrwxr-xr-x   1 root       sys             18 Nov 29  2005 /sbin/rc2.d/S393secsh -> /sbin/init.d/secsh

srvu0118:/sbin/rc2.d # /sbin/init.d/secsh
usage: /sbin/init.d/secsh {start|stop|start_msg|stop_msg}

srvu0118:/sbin/rc2.d # /sbin/init.d/secsh stop
HP-UX Secure Shell stopped

srvu0118:/sbin/rc2.d # /sbin/init.d/secsh start
HP-UX Secure Shell started

Concernant la configuration réseau, tout modifié efficacement avec SAM.
À REMARQUER TOUT DE MÊME la nécessité, pour la résolution de noms, de spécifier DNS AVANT /etc/hosts !
		(le 27 août 2010, je tombe sur le fichier SUPPORTS/AFNIC/guides/dns-intro/ClientConfig-HP-UX.html qui me confirme ce constat :
			Configuration d'une machine HP-UX utilisant le service de noms
				Ordre utilisé pour la recherche d'une adresse
					HP-UX utilise les mécanismes dans l'ordre suivant:
						1.	DNS, si configuré (présence d'un fichier /etc/resolv.conf
												ou de named sur la machine).
						2.	NIS, si configuré.
						3.	Fichier /etc/hosts)

ERREUR TOUT DE MÊME (à répétition) sur le changement de la passerelle par défaut :
│ UNEXPECTED EXIT: process LANG=C LC_ALL=C /usr/sam/lbin/samx -C -n -p │                                       
│ 2790 -s route /usr/sam/lib//route.ui exited with a non-zero exit     │                                       
│ status.                                                              │                                       
│                                                                      │                                       
│ sh: 2857 Memory fault(coredump)                                      │
==> Problème apparemment connu : http://forums13.itrc.hp.com/service/forums/questionanswer.do?admit=109447627+1263746880359+28353475&threadId=1188826
	--> "You need the latest SAM patch. This has nothing to do with networking."
Malgré les informations et consignes mentionnées dans le document ci-dessus, j'ai tout simplement pris l'initiative de changer la valeur de la variable ROUTE_GATEWAY[0]  dans le fichier approprié, ce qui donne :
# grep "^ROUTE_GATEWAY" /etc/rc.config.d/netconf
ROUTE_GATEWAY[0]=192.168.1.2

srvu0118:/etc # hpux_config						# invoque un script qui produit le rapport sauvé
												  dans le fichier hpux_config.srvu0118.txt

____________________________________________________________________________________________________

Je viens de réinitialiser le mot de passe root de l'autre machine (simplement "root" pour l'instant).

____________________________________________________________________________________________________
____________________________________________________________________________________________________

ORGANISATION MÉMOIRE :

L'installation des barrettes doit suivre un schéma précis (dont le détail est expliqué sur un autocollant fixé au-dessus du logement des cartes d'extension) :

	- Contrainte pour un serveur : n'installer les barrettes que par groupe de 4 (pas moins).

	- Normalement, le premier groupe devrait occuper les emplacements numérotés 0 et 1.
	  Le deuxième groupe devrait occuper les emplacements numérotés 2 et 3.
	  Enfin le troisième groupe devrait occuper les emplacements numérotés 4 et 5.

					LOGEMENT POUR CARTES D'EXTENSION

			--- DIMM 0B ---		--- DIMM 1B ---     A
A			--- DIMM 4B ---		--- DIMM 5B ---     R
V			--- DIMM 2B ---		--- DIMM 3B ---     R
A												    I
N		--- DIMM 0A ---				--- DIMM 1A --- E
T		--- DIMM 4A ---				--- DIMM 5A --- R
		--- DIMM 2A ---				--- DIMM 3A --- E

			PROCESSEURS

À NOTER : on ne constate pas de dysfonctionnement si l'on ne respecte pas scrupuleusement cette organisation. J'ai notamment rempli (par méconnaissance) les slots numérotés 0, 1, 4 et 5 et n'ai pas eu à en souffrir.
Je ne peux que SUPPOSER que l'organisation recommandée permet d'optimiser le flux d'air pour le refroidissement des barrettes.

Pour 4 barrettes :

					LOGEMENT POUR CARTES D'EXTENSION

			-=============-		-=============-     A
A			---------------		---------------     R
V			---------------		---------------     R
A												    I
N		-=============-				-=============- E
T		---------------				--------------- R
		---------------				--------------- E

			PROCESSEURS

Pour 8 barrettes :

					LOGEMENT POUR CARTES D'EXTENSION

			-=============-		-=============-     A
A			---------------		---------------     R
V			-=============-		-=============-     R
A												    I
N		-=============-				-=============- E
T		---------------				--------------- R
		-=============-				-=============- E

			PROCESSEURS

____________________________________________________________________________________________________
____________________________________________________________________________________________________

La machine détaillée ci-dessous est celle notée "B". (Voir plus haut machine "A".)

____

(Il semble que les ports série DB9 ne puissent pas être utilisés comme port "console".)

également "raccordable" (avec les identifiants mentionnés ci-après, Admin/Admin ou Oper/Oper) sur la prise série DB25 en 9600-N-8-1. (Consulter éventuellement "Default Console - hp integrity rx2600 Server - 5971-4238.pdf".)
Et, de fait, raccordé la première fois sur le port DB25   MAIS  avec une originalité, j'ai employé le cordon pieuvre spécifique (DB25 vers 3 DB9, "CONSOLE", "MODEM" et "UPS"). Bien entendu je me suis branché sur la DB9 nommée "CONSOLE".

Globalement les caractéristiques matérielles "fixes" sont les mêmes que pour la machine "A".

Remplacement des 4 Go d'origine (4 x 1 Go) par 4 Go achetés chez SQP (4 x 1 Go). C'est bon !

Autres tests :
8 Go SQP, ça NE marche sur AUCUNE des 2 machines.
4 Go HP + 4 Go SQP, ça semble fonctionner (les 8 Go sont reconnus).
4 Go HP OU 4 Go SQP, on a dit que c'était bon (voir juste un peu plus haut).
	=> BEN PAS VRAIMENT ! Quand on lance le test "MEMDIAG" sur un lot de 4 Go de RAM SQP (peut-être y-t-il un mélange de barrette correctes et d'autres défectueuses mais cela m'est difficile à déterminer), je constate des reboots à répétition.

Login Admin, mot de passe Admin.

[frbpcs52cons] MP:CM> lc

LC

At each prompt you may type DEFAULT to set default configuration or Q to Quit

Current LAN Configuration:
     - - MAC Address                : 0x0015608abab7
     D - DHCP Status                : Disabled
     I - IP Address                 : 10.3.142.137
     M - MP Host Name               : frbpcs52cons
     S - Subnet Mask                : 255.255.255.0
     G - Gateway Address            : 10.3.142.254
     L - Link State                 : Auto Negotiate
     W - Remote Serial Console Port : 2023
     - - SSH Access Port            : - (MP Feature Not Licensed)
     - - IPMI / LAN Port            : 623

___________________________________
___________________________________
___________________________________		24 avril 2010 :
___________________________________		CONCLUSION TEST DES RAM (échangées par SQP en avril 2010)
___________________________________

Les 4 x 4 barrettes de 1 Go (de marque hynix - voir photo "RAM hynix - OK.JPG") échangées ont passé avec succès plusieurs tests.
Physiquement elles se différencient (visiblement) principalement par leur épaisseur. En effet, les premières barrettes (incompatibles), étaient très épaisses et semblaient assemblées à partir de composants mémoire empilés l'un sur l'autre et de part à et d'autre du support (comme si au final il y avait 4 épaisseurs de composants). Les mémoires hynix se présentent elles de façon plus "traditionnelles".

___________________________________
___________________________________
___________________________________		18 décembre 2010 :
___________________________________		
___________________________________

J'ai changé la politique de renouvellement des mots de passe pour les utilisateurs root et laurent à l'aide du programme SAM. J'en ai désactivé l'expiration !

___________________________________
___________________________________
___________________________________		3 juillet 2011 :
___________________________________		
___________________________________

Modification adresses réseau.

	dans /etc/rc.config.d/netconf :
		modification adresse et "diffusion" de l'interface locale => 192.168.75.53 et 192.168.75.255
		modification adresse passerelle par défaut => 192.168.75.1

	dans /etc/resolv.conf :
		suppression d'une directive nameserver
		modification adresse de celle restante => 192.168.75.1

	dans /opt/ssh/etc/sshd_config :
		suppression de la directive "Port 22001"
		retrait de la marque de commentaire devant la directive "Port 22"